**DATE:** March 8, 2018

**SOLICITATION CHECKLIST**

**CONSULTANT ADMINISTRATION SECTION (CAS)**

**PROJECT NUMBERS:** NH-6-002(127)337; NH-6-002(128)342; NH-6-002(129)341

**PROJECT CONTROL NUMBERS:** 21980; 21981; 21982

**PROJECT DESCRIPTION:** US HWY 2

**DIVISION REPRESENTATIVE:** Robert Zahn **PHONE:** 328-2149

![C:\Users\abeise\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\S5QW37N8\MC900115855[2].gif]()

  **Consultant NDDOT N/A**

![C:\Users\abeise\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\S5QW37N8\MC900115855[2].gif]()

Any supporting documentation to CAS [ ]  [ ]  [ ]

**LiDAR**……………………………………………………………………………………. [x]  [ ]  [ ]

*Primary and Secondary Control as needed, Topographic Data and DTM Surface, LiDAR data in LAS format for both raw data and final processed data.*

**90-1 (SI) Safety Survey**…………………………………………………………..… [x]  [ ]  [ ]

*90-1 survey forms and other pertinent data, see attached requirements for 90-1.*

**90-1 Review**…………....…………………………………………………………...… [ ]  [x]  [ ]

*The NDDOT will complete the 90-1 safety review.*

**Bridge Survey**……………..….……………………………………………………………[x]  [ ]  [ ]

*Stream profile and cross sections as defined by the NDDOT bridge section and the completed SFN 3853 bridge survey form for the bridge structure 347.860 WB.*

**Ground Survey**…………..….……………………………………………………………[x]  [ ]  [ ]

*Define the median centerline alignment. PLSS corners are not required outside of the NDDOT right of way.*

**CADD Editing**……………..….……………………………………………………………[x]  [ ]  [ ]

*MicroStation drawings; Control (showing alignment), 081CD, Topog, DTM,*

This document needs to be signed if there are two Divisions with major portions of the project and one wants the work to go to a consultant and the other wants to keep the project.

Approval: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_

 Office of Project Development Director Date